Internal gear

Interference prevention

For no interference the following eq. must be satisfied

Where

p= pinion

G =gear

a= addendum radius

b=base radius